1 put the files (rom_h1_massto_nf1g.img and install.ss) into the usb flash disk's root directory
2 insert the usb flash disk into the set-top box
3 power on the set-top box
4 app is upgrading,please wait. The indicator on the usb flash disk will blinks
5 after upgrade is finined,the system will start up
6 please do not power off the STB during the whole proccess of updating.
7 After update you will find the software version is 103.
8 Connact the STB to internet and restart the STB and you will find an alarm "Updating the resource,please wait".
9 if the alrm "Updating the resource,please wait" not apear,please check the internat and restart the STB.
10 After you get the alarm,wait about five minute,and you will find the softeware version is 116.
